Copyright (C) 1997, 1998 by International Business Machines Corporation

# TCP/IP Configuration Notebook Online Help

### Changing a Remote Print Server and Attached Printer

To change a default remote print server (LPD) or attached printer to be used by this computer for LPR, LPQ, LPRM, and LPRMON commands:

1. Select the Printing tab.

2. Modify the host name entry of the server where you want your printer requests sent.

3. Modify the name of the print queue on the server, or the device name (such as LPT1) where you want your printer output printed. (If you specify a device name, the server will determine the queue.)

4. Click OK.

To change the maximum number of ports serviced by LPRPORTD:

1. Select the Printing tab.

2. Modify the maximum number of printer ports (from 2-64) to be serviced.

3. Click OK.

[ Top of Page | Previous Page | Next Page | Table of Contents ]